#

- Terminal Number
- Model Name
- Firmware version

- TOP
- Basic Setting
- Network Setting
- Create New Group
- Create New Caller
- Create New Eraser
- Connected Display Unit
- Other Setting
- Change Password

There is an error.

# Other Setting

## Volume Setting

Monitor output volume |

## Time Setting（NTP）

NTP synchronization | Sync Async
NTP Server |
Synchronization Interval |

## Time Setting（Manual）

Manual Setting |

## Caller(Model A) Setting

Long press time |

## Intermediate log output

Intermediate log output | Connect the USB serial converter to the USB terminal and connect to an external device. Communication settings ・baud rate：57600 bps ・data length：8 bit ・parity：なし ・stop bit：1 bit ・flow control：なし ・character code：UTF-8 ・line break：CR+LF

## Update Program

Firmware file |

## System Analysis（Download Internal Logs）

Download Internal Logs |

## Restore factory settings

Restore factory settings |
Registration information output |
Enter registration information | Restore network settings（including Wi-Fi information）

## Specific Setting

SSH（temporary） |
Log Level（internal logs） |
Initialise data |
Restart |